# Reliability Calculation Result

λref \* Pi\_S \* Pi\_U \* Pi\_I \* Pi\_T \* Pi\_E

Component λref= 200.0

Component type :1-pole DC contractors

Pi\_S Value is Constant

Component Pi\_S= 1

Component Pi\_U= 1

Component Operating voltage U in V :≤ 200

Component Pi\_I= 0.15

Component Current ratio (I/Ie) :0.33

Pi\_T Value is Constant

Component Pi\_T= 1

Pi\_E Value is Constant

Component Pi\_E= 1

λ = 200.0 \* 1 \* 1 \* 0.15 \* 1 \* 1

λ = 30.0